DEFALT  , Configure.General  , Default Settings  , DEFCMD  , Recover Default Settings  ,0,0,0,0, N  , N  ,configure_general.htm#recover_default_settings
REV_SW  , Configure.General  , Software Revision  , EDIT_READONLY  , Revisions  ,0,0, N/A  ,0, N  , N  ,configure_general.htm#revisions
REV_WA  , Configure.General  , Software Part Number  , EDIT_READONLY  , Revisions  ,0,0, N/A  ,0, N  , N  ,configure_general.htm#revisions
REV_TD  , Configure.General  , Software Time-Date Stamp  , EDIT_READONLY  , Revisions  ,0,0, N/A  ,0, N  , N  ,configure_general.htm#revisions
ENGREV	, Configure.General  , Engine Revision  , EDIT_READONLY  , Revisions  ,0,0, N/A ,0, N  , N  ,configure_general.htm#revisions
IMGMXX  , Configure.General  , Horizontal Pixels  , EDIT  , Image Characteristics  ,0,0,640,0, N  , N  ,configure_general.htm#image_characteristics
IMGMXY  , Configure.General  , Vertical Pixels  , EDIT  , Image Characteristics  ,0,0,480,0, N  , N  ,configure_general.htm#image_characteristics
IMGBPP  , Configure.General  , Image Bits Per Pixel  , EDIT_READONLY  , Image Characteristics  ,0,0,8,0, N  , N  ,configure_general.htm#image_characteristics
TSTMNU  , Configure.General  , Test Menu  , CHECK  , Diagnostics  ,0,1,0,0, N  , N  ,configure_general.htm#diagnostics
VIDREV  , Configure.Scanning Options  , Decode Reverse Video Images  , CHECK  , Other  ,0,1,0,0, N  , N  ,configure_scanning_options.htm#other
SCNLED  , Configure.Scanning Options  , Illumination Lights, CHECK  , Scanner / Illumination Lights,0,1,1,0, N  , N  ,configure_scanning_options.htm#scanner_/_illumination_lights
DECWIN  , Configure.Scanning Options  , Centering On  , CHECK  , Centering  ,0,1,0,0, N  , N  ,configure_scanning_options.htm#centering
DECTOP  , Configure.Scanning Options  , Top Of Centering Window  , EDIT  , Centering  ,0,100,40,0, N  , N  ,configure_scanning_options.htm#centering
DECBOT  , Configure.Scanning Options  , Bottom Of Centering Window  , EDIT  , Centering  ,0,100,60,0, N  , N  ,configure_scanning_options.htm#centering
DECLFT  , Configure.Scanning Options  , Left Of Centering Window  , EDIT  , Centering  ,0,100,40,0, N  , N  ,configure_scanning_options.htm#centering
DECRGT  , Configure.Scanning Options  , Right Of Centering Window  , EDIT  , Centering  ,0,100,60,0, N  , N  ,configure_scanning_options.htm#centering
DECMOD  , Configure.Scanning Options  , Decode Mode  , RADIO1  , None  ,0,0, Full Omnidirectional  ,Full Omnidirectional|Quick Omnidirectional|Advanced Linear Decoding| N/A  , N  , N  ,configure_scanning_options.htm#decode_mode
SHOTGN  , Configure.Scanning Options  , Multiple Symbols  , CHECK  , Decoding  ,0,1,0,0, N  , N  ,configure_scanning_options.htm#decoding
SHWNRD  , Configure.Scanning Options  , Show 'No Read'  , CHECK  , Decoding  ,0,1,0,0, N  , N  ,configure_scanning_options.htm#decoding
PRTWGT  , Configure.Scanning Options  , Print Weight  , EDIT  , Decoding  ,1,7,4,0, N  , N  ,configure_scanning_options.htm#decoding
//Inserted here below(for 1284)
ROTATN  , Configure.Scanning Options  , Working Orientation  , RADIO1  , None  ,0,0, Upright  , Upright | Rotate Clockwise 90 Degrees | Upside Down | Rotate Counterclockwise 90 Degrees  , N  , N  ,configure_scanning_options.htm#working_orientation
PRFDFT  , Configure.Scanning Options  , Default,	DEFCMD,	Preferred Symbologies,	0,0,0,0,N,Y,configure_scanning_options.htm#preferredsymbologies
PRFENA  , Configure.Scanning Options  , Enable,	CHECK,	Preferred Symbologies,	0,1,0,0,N,N,configure_scanning_options.htm#preferredsymbologies
PRFPTO  , Configure.Scanning Options  , High Priority Timeout (ms),	EDIT,	Preferred Symbologies,	1,10000,500,0,N,N,configure_scanning_options.htm#preferredsymbologies
// next 2 commented out per bug 4379
//PRFCOD  , Configure.Scanning Options  , High Priority Symbology, BLOCK,  Preferred Symbologies,  0,0,ffff,0,N,N,configure_scanning_options.htm#preferredsymbologies
//PRFBLK  , Configure.Scanning Options  , Low Priority Symbologies, BLOCK, Preferred Symbologies,  0,0,ffff,0,N,N,configure_scanning_options.htm#preferredsymbologies
TRGMOD  , Configure.Device Settings, Trigger Mode  , RADIO1  , None  ,0,0, Manual/Serial  ,Manual/Serial|N/A|Manual Low Power|Presentation Mode|Scan Stand Mode| N/A| N/A| N/A|Streaming Presentation(TM) Mode  , N  , N  ,configure_device_settings.htm#trigger_mode
TRGSSW  , Configure.Device Settings, Enable,CHECK,In-Stand Sensor Mode,0,1,0,0,N,N,configure_device_settings.htm#in_stand_sensor_mode
TRGSTO  , Configure.Device Settings,Read Time-out (milliseconds)  , EDIT  , Manual/Serial Trigger  ,0,300000,30000,0, N  , N  ,configure_device_settings.htm#manual/serial_trigger
TRGPTO  , Configure.Device Settings, Hands Free Time-out (milliseconds)  , EDIT  , Hands Free Time-out  ,0,300000,5000,0, N  , N  ,configure_device_settings.htm#hands_free_time-out
TRGLPT  , Configure.Device Settings, Low Power Time-Out (sec)  , EDIT  , Low Power  ,0,300,120,0, N  , N  ,configure_device_settings.htm#low_power
SCNDLY  , Configure.Device Settings, Aimer Delay (ms)  , EDIT  , Aimer Control  ,0,4000,0,0, N  , N  ,configure_device_settings.htm#aimer_control
SCNAIM  , Configure.Device Settings, Aimer Mode  , RADIO1  , Aimer Control  ,0,0, Concurrent  ,Off|Concurrent| Interlaced  , N  , N  ,configure_device_settings.htm#aimer_control
SDRTIM  , Configure.Device Settings, Read Time-out (ms)  , EDIT  , Imager Time-out After Untrigger  ,0,999999,60000,0, N  , N  ,configure_device_settings.htm#imager_time-out_after_untrigger
DLYRRD  , Configure.Device Settings, Re-read Delay (handsfree mode only) (ms)  , EDIT  , Decoding Delay  ,0,30000,750,0, N  , Y  ,configure_device_settings.htm#decoding_delay
DLYGRD  , Configure.Device Settings, Good Read Delay (ms)  , EDIT  , Decoding Delay  ,0,30000,0,0, N  , Y  ,configure_device_settings.htm#decoding_delay
PWRLDC  , Configure.Device Settings, LED Duty Cycle  , EDIT  , Power  ,0,100,100,0, N  , N  ,configure_device_settings.htm#led_duty_cycle
TRGPCK, Configure.Device Settings,Presentation LED Behavior After Decode,CHECK,Presentation Mode Modifiers,0,1,1,0, N  , N  ,configure_device_settings.htm#presentation_mode_modifiers
TRGPMS, Configure.Device Settings,Presentation Sensitivity,EDIT,Presentation Mode Modifiers,0,20,1,0,N,N,configure_device_settings.htm#presentation_mode_modifiers
WNDPOL  , Configure.Wand/Laser Emulation  , Wand Emulation Output Polarity  , RADIO1  , None  ,0,0, Black High  ,Black High| White High  , N  , Y  ,configure_wand_laser_emulation.htm#wand_emulation_output_polarity
WNDSPD  , Configure.Wand/Laser Emulation  , Wand Emulation Transmission Rate (in/sec)  , RADIO2  , None  ,0,0,25,10|25|40|80|120|150|200  , N  , Y  ,configure_wand_laser_emulation.htm#wand_emulation_transmission_rate_(in/sec)
WNDIDL  , Configure.Wand/Laser Emulation  , Wand Emulation Idle State  , RADIO1  , None  ,0,0, High  ,Low| High  , N  , Y  ,configure_wand_laser_emulation.htm#wand_emulation_idle_state
WNDCHK  , Configure.Wand/Laser Emulation  , Overall Checksum On  , CHECK  , Wand Emulation  ,0,1,0,0, N  , N  ,configure_wand_laser_emulation.htm#wand_emulation
WNDBLK  , Configure.Wand/Laser Emulation  , Data Block Size  , RADIO1  , Wand Emulation  ,0,0, 40 Characters  ,20 Characters|40 Characters|60 Characters| 80 Characters  , N  , Y  ,configure_wand_laser_emulation.htm#wand_emulation
WNDDLY  , Configure.Wand/Laser Emulation  , Delay Between Blocks  , RADIO1  , Wand Emulation  ,0,0, 50 ms  ,5 ms|50 ms|150 ms| 500 ms  , N  , Y  ,configure_wand_laser_emulation.htm#wand_emulation
KBDCTY  , Configure.Keyboard Wedge  , Keyboard Country  , COMBOBOX  , None  ,0,0, United States  ,United States|Belgium|Finland (Sweden)|France|Germany|Italy|Switzerland|United Kingdom|Denmark|Norway|Spain|Dutch|Hebrew|Portugal|LatinAmerica|Czech|N/A|Greek|French Canada|Hungary|Poland|SCS|Slovak|Sweden|Turkey Q|Romania|Russia| Turkey F|Japan ASCII|Switzerland French|  USA International|Slovenia|Croatia|Bosnia|Macedonia|Albania|Serbia Latin|Serbia Cyrillic|Czech Qwertz|Czech Qwerty|  Czech Programmers|Estonia|Latvia|Latvia Qwerty|Lithuania|Lithuanian IBM|N/A|N/A|Slovak Qwertz|Slovak Qwerty|  Hungarian 101 Key|Spanish Variation|Bulgaria Cyrillic|Bulgaria Latin|Canadian French Legacy|Canadian Multilingual|Italian 142|Polish 214|Polish Programmers|Brazil MS|  Greek Polytonic|Greek 220|Greek 319|Greek Latin|Greek 220 Latin|Greek 319 Latin|Greek MS|Russian MS|Russian Typewriter|N/A|  N/A|N/A|N/A|Ireland|Malta|Iceland|Ukraine|Uzbek Cyrillic|Kazakh|Kyrgyz Cyrillic|  Azeri Latin|AzeriCyrillic|Belarusian|Faeroese|Gaelic|Tatar|Mongolian Cyrillic|USA Dvorak|USA Dvorak Lefthand|USA Dvorak Righthand,N,Y,configure_keyboard_wedge.htm#keyboard_country
KBDSTY  , Configure.Keyboard Wedge  , Keyboard Style  , RADIO2  , None  ,0,0, Regular  ,Regular|Caps Lock|Shift Lock|N/A|N/A|Emulate External Keyboard|Auto CAPS lock| Auto CAPS lock via Numpad  , N  , Y  ,configure_keyboard_wedge.htm#keyboard_style
KBDADC  , Configure.Keyboard Wedge  , Auto Direct Connect  , CHECK  , Keyboard Modifiers  ,0,1,0,0, N  , Y  ,configure_keyboard_wedge.htm#keyboard_modifiers
KBDNPS  , Configure.Keyboard Wedge  , Numeric Keypad  , CHECK  , Keyboard Modifiers  ,0,1,0,0, N  , Y  ,configure_keyboard_wedge.htm#keyboard_modifiers
KBDTMD  , Configure.Keyboard Wedge  , Turbo  , CHECK  , Keyboard Modifiers  ,0,1,0,0, N  , Y  ,configure_keyboard_wedge.htm#keyboard_modifiers
KBDCAS  , Configure.Keyboard Wedge  , Crtl + ASCII  , RADIO1  , Keyboard Modifiers  ,0,0, Off  , Off|DOS|Windows  , N  , Y  ,configure_keyboard_wedge.htm#keyboard_modifiers
KBDDED  , Configure.Keyboard Wedge  , Dead Key Translation  , CHECK  , International  ,0,1,1,0, N  , Y  ,configure_keyboard_wedge.htm#international
KBDALT  , Configure.Keyboard Wedge  , Dead Key Thru Alt+Numpad Sequence  , RADIO1  , International  ,0,0, Disabled  ,Disabled|Windows Style| DOS Style|Unicode|Windows System Code Page|DOS System Code Page  , N  , Y  ,configure_keyboard_wedge.htm#international
KBDDFT  , Configure.Keyboard Wedge  , Default All Options  , DEFCMD  , Keyboard Options  ,0,0,0,0, N  , Y  ,configure_keyboard_wedge.htm#keyboard_options
// IMGVGA must come first because when this is enabled or disbled the IMGWNR, WNL, WNT, WNB are reset
IMGVGA  , Configure.Image Transfer Options, Force VGA Resolution  , CHECK  , Image Ship Default Parameters  ,0,1,1,0, N  , N  ,configure_image_transfer_options.htm#image_ship_default_parameters
IMGCOR  , Configure.Image Transfer Options, Compensation Enabled  , CHECK  , Image Ship Default Parameters  ,0,1,0,0, N  , N  ,configure_image_transfer_options.htm#image_ship_default_parameters
IMGEDG  , Configure.Image Transfer Options, Sharpen Edges, EDIT  , Image Ship Default Parameters  ,0,23,0,0, N  , N  ,configure_image_transfer_options.htm#image_ship_default_parameters
IMGFMT  , Configure.Image Transfer Options, File Format  , RADIO1  , Image Ship Default Parameters  ,0,0, JPEG  , KIM|TIFF Binary|TIFF Binary Group 4 Compressed|TIFF Grayscale|Uncompressed Binary|Uncompressed Grayscale|JPEG|N/A|BMP  , N  , N  ,configure_image_transfer_options.htm#image_ship_default_parameters
IMGHIS  , Configure.Image Transfer Options, Histogram Stretch Enabled  , CHECK  , Image Ship Default Parameters  ,0,1,0,0, N  , N  ,configure_image_transfer_options.htm#image_ship_default_parameters
IMGNVX  , Configure.Image Transfer Options, Invert Around X Axis Enabled  , CHECK  , Image Ship Default Parameters  ,0,1,0,0, N  , N  ,configure_image_transfer_options.htm#image_ship_default_parameters
IMGNVY  , Configure.Image Transfer Options, Invert Around Y Axis Enabled  , CHECK  , Image Ship Default Parameters  ,0,1,0,0, N  , N  ,configure_image_transfer_options.htm#image_ship_default_parameters
IMGJQF  , Configure.Image Transfer Options, JPEG Image Quality  , EDIT  , Image Ship Default Parameters  ,0,100,50,0, N  , N  ,configure_image_transfer_options.htm#image_ship_default_parameters
IMGGAM  , Configure.Image Transfer Options, Gamma Correction  , EDIT  , Image Ship Default Parameters  ,0,1000,0,0, N  , N  ,configure_image_transfer_options.htm#image_ship_default_parameters
IMGWNL  , Configure.Image Transfer Options, Image Cropping Left Edge  , EDIT  , Image Ship Default Parameters  ,0,639,0,0, N  , N  ,configure_image_transfer_options.htm#image_ship_default_parameters
IMGWNR  , Configure.Image Transfer Options, Image Cropping Right Edge  , EDIT  , Image Ship Default Parameters  ,0,639,639,0, N  , N  ,configure_image_transfer_options.htm#image_ship_default_parameters
IMGWNT  , Configure.Image Transfer Options, Image Cropping Top Edge  , EDIT  , Image Ship Default Parameters  ,0,479,0,0, N  , N  ,configure_image_transfer_options.htm#image_ship_default_parameters
IMGWNB  , Configure.Image Transfer Options, Image Cropping Bottom Edge  , EDIT  , Image Ship Default Parameters  ,0,479,479,0, N  , N  ,configure_image_transfer_options.htm#image_ship_default_parameters
IMGMAR  , Configure.Image Transfer Options, Image Cropping Margin  , EDIT  , Image Ship Default Parameters  ,0,240,0,0, N  , N  ,configure_image_transfer_options.htm#image_ship_default_parameters
IMGXFR  , Configure.Image Transfer Options, Protocol  , RADIO1  , Image Ship Default Parameters  ,0,0, HModem Compressed  , None|N/A|No HModem|HModem Compressed|HModem Uncompressed  , N  , N  ,configure_image_transfer_options.htm#image_ship_default_parameters
IMGSUB  , Configure.Image Transfer Options, Pixel Ship  , EDIT  , Image Ship Default Parameters  ,1,10,1,0, N  , N  ,configure_image_transfer_options.htm#image_ship_default_parameters
IMGUSH  , Configure.Image Transfer Options, Document Image Filter  , EDIT  , Image Ship Default Parameters  ,0,255,0,0, N  , N  ,configure_image_transfer_options.htm#image_ship_default_parameters
IMGHST  , Configure.Image Transfer Options, Histogram Enabled  , CHECK  , Image Ship Default Parameters  ,0,1,0,0, N  , N  ,configure_image_transfer_options.htm#image_ship_default_parameters
IMGINF  , Configure.Image Transfer Options, Infinity Filter Enabled  , CHECK  , Image Ship Default Parameters  ,0,1,0,0, N  , N  ,configure_image_transfer_options.htm#image_ship_default_parameters
IMGROT  , Configure.Image Transfer Options, Rotation  , RADIO1  , Image Ship Default Parameters  ,0,0, Upright  , Upright | Rotate Clockwise 90 Degrees | Upside Down | Rotate Counterclockwise 90 Degrees  , N  , N  ,configure_image_transfer_options.htm#image_ship_default_parameters
IMGDFT  , Configure.Image Transfer Options, Default  , DEFCMD  , Image Ship  ,0,0,0,0, N  , N  ,configure_image_transfer_options.htm#image_ship
SNPSTY  , Configure.Image Transfer Options, Imaging Style  , RADIO1  , Image Snap Default Parameters  ,0,0, Photo  , Decoding|Photo|Manual  , N  , N  ,configure_image_transfer_options.htm#image_snap_default_parameters
SNPDEL  , Configure.Image Transfer Options, Delta For Acceptance  , EDIT  , Image Snap Default Parameters  ,0,100,25,0, N  , N  ,configure_image_transfer_options.htm#image_snap_default_parameters
SNPLED  , Configure.Image Transfer Options, LED State  , RADIO1  , Image Snap Default Parameters  ,0,0, Off  , Off|On|N/A  , N  , N  ,configure_image_transfer_options.htm#image_snap_default_parameters
SNPTRY  , Configure.Image Transfer Options, Update Tries  , EDIT  , Image Snap Default Parameters  ,0,10,6,0, N  , N  ,configure_image_transfer_options.htm#image_snap_default_parameters
SNPWHT  , Configure.Image Transfer Options, Target White Value  , EDIT  , Image Snap Default Parameters  ,1,255,125,0, N  , N  ,configure_image_transfer_options.htm#image_snap_default_parameters
SNPEXP  , Configure.Image Transfer Options, Exposure  , EDIT  , Image Snap Default Parameters  ,1,7874,7874,0, N  , N  ,configure_image_transfer_options.htm#image_snap_default_parameters
SNPGAN  , Configure.Image Transfer Options, Gain  , EDIT  , Image Snap Default Parameters  ,1,8,1,0, N  , N  ,configure_image_transfer_options.htm#image_snap_default_parameters
SNPPCT  , Configure.Image Transfer Options, Target Set Point Percentage  , EDIT  , Image Snap Default Parameters  ,1,99,50,0, N  , N  ,configure_image_transfer_options.htm#image_snap_default_parameters
SNPBEP  , Configure.Image Transfer Options, Beep After Snap  , CHECK  , Image Snap Default Parameters  ,0,1,0,0, N  , N  ,configure_image_transfer_options.htm#image_snap_default_parameters
SNPTRG  , Configure.Image Transfer Options, Wait For Trigger  , CHECK  , Image Snap Default Parameters  ,0,1,0,0, N  , N  ,configure_image_transfer_options.htm#image_snap_default_parameters
BEPBIP  , Configure.Output  , Beeper Duration - Short  , CHECK  , Beeper  ,0,1,0,0, N  , N  ,configure_output.htm#beeper
BEPRPT  , Configure.Output  , Number of Beeps per Good Read  , EDIT  , Beeper  ,1,9,1,0, N  , N  ,configure_output.htm#beeper
BEPBEP  , Configure.Output  , Beep On Good Read  , CHECK  , Beeper  ,0,1,1,0, N  , N  ,configure_output.htm#beeper
BEPFQ1  , Configure.Output  , Good Read Beep Frequency  , EDIT  , Beeper  ,400,9000,3250,0, N  , N  ,configure_output.htm#beeper
BEPLVL  , Configure.Output  , Volume  , RADIO1  , Beeper  ,0,0, Medium  ,Off|Low|Medium| High  , N  , N  ,configure_output.htm#beeper
BEPLED  , Configure.Output  , Good Read LED  , CHECK  , LED  ,0,1,1,0, N  , N  ,configure_output.htm#led
DLYCHR  , Configure.Output  , Intercharacter ( x 5ms)  , EDIT  , Output Delay  ,0,99,0,0, N  , N  ,configure_output.htm#output_delay
DLYFNC  , Configure.Output  , Interfunction ( x 5ms)  , EDIT  , Output Delay  ,0,99,0,0, N  , N  ,configure_output.htm#output_delay
DLYMSG  , Configure.Output  , Intermessage ( x 5ms)  , EDIT  , Output Delay  ,0,99,0,0, N  , N  ,configure_output.htm#output_delay
RMVFNC  , Configure.Output  , Remove Function Codes  , CHECK  , Embedded Function Codes  ,0,1,0,0, N  , N  ,configure_output.htm#embedded_function_codes
2IF_EN  , Configure.Output  , On  , CHECK  , Secondary Interface  ,0,1,0,0, N  , N  ,configure_output.htm#secondary_interface
2IFTRG  , Configure.Output  , Trigger Mode  , RADIO1  , Secondary Interface  ,0,3, Manual  ,Manual|N/A|Manual Low Power|Presentation Mode|Scan Stand Mode| N/A  , N  , N  ,configure_output.htm#secondary_interface
2IFLPT  , Configure.Output  , Low Power Time-Out (sec)  , EDIT  , Secondary Interface  ,0,1,120,0, N  , N  ,configure_output.htm#secondary_interface
2IFTYP  , Configure.Output  , Interface Type  , COMBOBOX  , Secondary Interface  ,0,0, RS-232  ,RS-232|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|     N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|     N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|     N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|     N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|     N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|     N/A|Wand Emulation Code 39|N/A|N/A|Wand Emulation Same Code|N/A|N/A|N/A|N/A|N/A|     N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|     N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A   , N  , Y  ,configure_output.htm#secondary_interface
SEQBLK  , Configure.Data Format , Sequence  , BLOCK  , Output Sequence  ,0,0, ffff  ,0, N  , N  ,configure_data_format.htm#output_sequence
SEQ_EN  , Configure.Data Format , Output Sequence Mode  , RADIO1  , None  ,0,0, Disabled  ,Disabled|Enabled| Enabled/Required  , N  , N  ,configure_data_format.htm#output_sequence_mode
C11ENA  , Configure.Symbologies.Linear.Code 11/128/39, Decoding On  , CHECK  , Code 11  ,0,1,0,0, N  , N  ,configure_symbologies_linear_code_11_128_39.htm#code_11
C11CK2  , Configure.Symbologies.Linear.Code 11/128/39, Two Check Digits  , CHECK  , Code 11  ,0,1,1,0, N  , N  ,configure_symbologies_linear_code_11_128_39.htm#code_11
C11MIN  , Configure.Symbologies.Linear.Code 11/128/39, Minimum Length  , EDIT  , Code 11  ,1,80,4,0, N  , N  ,configure_symbologies_linear_code_11_128_39.htm#code_11
C11MAX  , Configure.Symbologies.Linear.Code 11/128/39, Maximum Length  , EDIT  , Code 11  ,1,80,80,0, N  , N  ,configure_symbologies_linear_code_11_128_39.htm#code_11
C11DFT  , Configure.Symbologies.Linear.Code 11/128/39, Default  , DEFCMD  , Code 11  ,0,0,0,0, N  , N  ,configure_symbologies_linear_code_11_128_39.htm#code_11
128ENA  , Configure.Symbologies.Linear.Code 11/128/39, Decoding On  , CHECK  , Code 128  ,0,1,1,0, N  , N  ,configure_symbologies_linear_code_11_128_39.htm#code_128
128FNX  , Configure.Symbologies.Linear.Code 11/128/39, Function Code Transmit  , CHECK  , Code 128  ,0,1,0,0, N  , N  ,configure_symbologies_linear_code_11_128_39.htm#code_128
ISBENA  , Configure.Symbologies.Linear.Code 11/128/39, ISBT Decoding On  , CHECK  , Code 128  ,0,1,0,0, N  , N  ,configure_symbologies_linear_code_11_128_39.htm#code_128
128MIN  , Configure.Symbologies.Linear.Code 11/128/39, Minimum Length  , EDIT  , Code 128  ,0,80,0,0, N  , N  ,configure_symbologies_linear_code_11_128_39.htm#code_128
128MAX  , Configure.Symbologies.Linear.Code 11/128/39, Maximum Length  , EDIT  , Code 128  ,0,80,80,0, N  , N  ,configure_symbologies_linear_code_11_128_39.htm#code_128
128DFT  , Configure.Symbologies.Linear.Code 11/128/39, Default  , DEFCMD  , Code 128  ,0,0,0,0, N  , N  ,configure_symbologies_linear_code_11_128_39.htm#code_128
128DCP  , Configure.Symbologies.Linear.Code 11/128/39, Code Page  , COMBOBOX  , Code 128 Code Page  ,0,0, ISO 2022 Auto  ,N/A|ASCII - USA (ISO 2022-6/ISO646)|ISO 2022 Auto|N/A|N/A|N/A|N/A|N/A|N/A|N/A|   N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|    N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|ISO 8859-1|ISO 8859-2|ISO 8859-3|ISO 8859-4|ISO 8859-5|ISO 8859-6|ISO 8859-7|ISO 8859-8|ISO 8859-9|ISO 8859-10|ISO 8859-11|ISO 8859-12|ISO 8859-13|ISO 8859-14|ISO 8859-15|N/A|N/A|N/A|N/A|KIO8-U (Ukraine)|KIO8-R (Russian)|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|ISO 2022-25 (France / Belgium)|ISO 2022-11 (Sweden)|ISO 2022-69 (France / Belgium)|ISO 2022-21 (Germany)|ISO 2022-15 (Italy)|ISO 2022-xx (Switzerland)|ISO 2022-04 (UK)|ISO 2022-xx (Denmark)|ISO 2022-61 (Norway)|ISO 2022-17 (Spain), N  , N  ,configure_symbologies_linear_code_11_128_39.htm#code_128_code_page
C39ENA  , Configure.Symbologies.Linear.Code 11/128/39, Decoding On  , CHECK  , Code 39  ,0,1,1,0, N  , N  ,configure_symbologies_linear_code_11_128_39.htm#code_39
C39SSX  , Configure.Symbologies.Linear.Code 11/128/39, Transmit Start/Stop Characters  , CHECK  , Code 39  ,0,1,0,0, N  , N  ,configure_symbologies_linear_code_11_128_39.htm#code_39
C39CK2  , Configure.Symbologies.Linear.Code 11/128/39, Check Character  , RADIO1  , Code 39  ,0,0, No Check Character  ,No Check Character|Validate but Don't Transmit| Validate and Transmit  , N  , N  ,configure_symbologies_linear_code_11_128_39.htm#code_39
C39APP  , Configure.Symbologies.Linear.Code 11/128/39, Append Mode  , CHECK  , Code 39  ,0,1,0,0, N  , N  ,configure_symbologies_linear_code_11_128_39.htm#code_39
C39ASC  , Configure.Symbologies.Linear.Code 11/128/39, Full ASCII Mode  , CHECK  , Code 39  ,0,1,0,0, N  , N  ,configure_symbologies_linear_code_11_128_39.htm#code_39
C39B32  , Configure.Symbologies.Linear.Code 11/128/39, Code 32 (PARAF) Decoding On  , CHECK  , Code 39  ,0,1,0,0, N  , N  ,configure_symbologies_linear_code_11_128_39.htm#code_39
C39MIN  , Configure.Symbologies.Linear.Code 11/128/39, Minimum Length  , EDIT  , Code 39  ,0,48,0,0, N  , N  ,configure_symbologies_linear_code_11_128_39.htm#code_39
C39MAX  , Configure.Symbologies.Linear.Code 11/128/39, Maximum Length  , EDIT  , Code 39  ,0,48,48,0, N  , N  ,configure_symbologies_linear_code_11_128_39.htm#code_39
C39DFT  , Configure.Symbologies.Linear.Code 11/128/39, Default  , DEFCMD  , Code 39  ,0,0,0,0, N  , N  ,configure_symbologies_linear_code_11_128_39.htm#code_39
C39DCP  , Configure.Symbologies.Linear.Code 11/128/39, Code Page  , COMBOBOX  , Code 39 Code Page  ,0,0, ISO 2022 Auto  ,N/A|ASCII - USA (ISO 2022-6/ISO646)|ISO 2022 Auto|N/A|N/A|N/A|N/A|N/A|N/A|N/A|    N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|    N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|ISO 8859-1|ISO 8859-2|ISO 8859-3|ISO 8859-4|ISO 8859-5|ISO 8859-6|ISO 8859-7|ISO 8859-8|ISO 8859-9|ISO 8859-10|ISO 8859-11|ISO 8859-12|ISO 8859-13|ISO 8859-14|ISO 8859-15|N/A|N/A|N/A|N/A|KIO8-U (Ukraine)|KIO8-R (Russian)|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|ISO 2022-25 (France / Belgium)|ISO 2022-11 (Sweden)|ISO 2022-69 (France / Belgium)|ISO 2022-21 (Germany)|ISO 2022-15 (Italy)|ISO 2022-xx (Switzerland)|ISO 2022-04 (UK)|ISO 2022-xx (Denmark)|ISO 2022-61 (Norway)|ISO 2022-17 (Spain), N  , N  ,configure_symbologies_linear_code_11_128_39.htm#code_39_code_page
CBRENA  , Configure.Symbologies.Linear.Codabar/Code 93, Decoding On  , CHECK  , Codabar F,0,1,1,0, N  , N  ,configure_symbologies_linear_codabar_code_93.htm#codabar_f
CBRSSX  , Configure.Symbologies.Linear.Codabar/Code 93, Transmit Start/Stop Characters  , CHECK  , Codabar F,0,1,0,0, N  , N  ,configure_symbologies_linear_codabar_code_93.htm#codabar_f
CBRMIN  , Configure.Symbologies.Linear.Codabar/Code 93, Minimum Length  , EDIT  , Codabar F,2,60,4,0, N  , N  ,configure_symbologies_linear_codabar_code_93.htm#codabar_f
CBRMAX  , Configure.Symbologies.Linear.Codabar/Code 93, Maximum Length  , EDIT  , Codabar F,2,60,60,0, N  , N  ,configure_symbologies_linear_codabar_code_93.htm#codabar_f
CBRCK2  , Configure.Symbologies.Linear.Codabar/Code 93, Check Character  , RADIO1  , Codabar F,0,0, No Check Character  ,No Check Character|Validate MOD 16 - No Transmit| Validate MOD 16 - Transmit  , N  , N  ,configure_symbologies_linear_codabar_code_93.htm#codabar_f
CBRCCT  , Configure.Symbologies.Linear.Codabar/Code 93, Concatenation  , RADIO2  , Codabar F,0,0, Off  ,Off|On| Required  , N  , N  ,configure_symbologies_linear_codabar_code_93.htm#codabar_f
CBRDFT  , Configure.Symbologies.Linear.Codabar/Code 93, Default  , DEFCMD  , Codabar F,0,0,0,0, N  , N  ,configure_symbologies_linear_codabar_code_93.htm#codabar_f
C93ENA  , Configure.Symbologies.Linear.Codabar/Code 93, Decoding On  , CHECK  , Code 93  ,0,1,1,0, N  , N  ,configure_symbologies_linear_codabar_code_93.htm#code_93
C93MIN  , Configure.Symbologies.Linear.Codabar/Code 93, Minimum Length  , EDIT  , Code 93  ,0,80,0,0, N  , N  ,configure_symbologies_linear_codabar_code_93.htm#code_93
C93MAX  , Configure.Symbologies.Linear.Codabar/Code 93, Maximum Length  , EDIT  , Code 93  ,0,80,80,0, N  , N  ,configure_symbologies_linear_codabar_code_93.htm#code_93
C93DFT  , Configure.Symbologies.Linear.Codabar/Code 93, Default  , DEFCMD  , Code 93  ,0,0,0,0, N  , N  ,configure_symbologies_linear_codabar_code_93.htm#code_93
C93DCP  , Configure.Symbologies.Linear.Codabar/Code 93, Code Page  , COMBOBOX  , Code 93 Code Page  ,0,0, ISO 2022 Auto  ,N/A|ASCII - USA (ISO 2022-6/ISO646)|ISO 2022 Auto|N/A|N/A|N/A|N/A|N/A|N/A|N/A|    N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|    N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|ISO 8859-1|ISO 8859-2|ISO 8859-3|ISO 8859-4|ISO 8859-5|ISO 8859-6|ISO 8859-7|ISO 8859-8|ISO 8859-9|ISO 8859-10|ISO 8859-11|ISO 8859-12|ISO 8859-13|ISO 8859-14|ISO 8859-15|N/A|N/A|N/A|N/A|KIO8-U (Ukraine)|KIO8-R (Russian)|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|ISO 2022-25 (France / Belgium)|ISO 2022-11 (Sweden)|ISO 2022-69 (France / Belgium)|ISO 2022-21 (Germany)|ISO 2022-15 (Italy)|ISO 2022-xx (Switzerland)|ISO 2022-04 (UK)|ISO 2022-xx (Denmark)|ISO 2022-61 (Norway)|ISO 2022-17 (Spain), N  , N  ,configure_symbologies_linear_codabar_code_93.htm#code_93_code_page
UPAENA  , Configure.Symbologies.Linear.UPC Codes, Decoding On  , CHECK  , UPC-A  ,0,1,1,0, N  , N  ,configure_symbologies_linear_upc_codes.htm#upc-a
UPACKX  , Configure.Symbologies.Linear.UPC Codes, Check Digit Transmit  , CHECK  , UPC-A  ,0,1,1,0, N  , N  ,configure_symbologies_linear_upc_codes.htm#upc-a
UPANSX  , Configure.Symbologies.Linear.UPC Codes, Number System Digit Transmit  , CHECK  , UPC-A  ,0,1,1,0, N  , N  ,configure_symbologies_linear_upc_codes.htm#upc-a
UPAAD2  , Configure.Symbologies.Linear.UPC Codes, 2 Digit Addenda  , CHECK  , UPC-A  ,0,1,0,0, N  , N  ,configure_symbologies_linear_upc_codes.htm#upc-a
UPAAD5  , Configure.Symbologies.Linear.UPC Codes, 5 Digit Addenda  , CHECK  , UPC-A  ,0,1,0,0, N  , N  ,configure_symbologies_linear_upc_codes.htm#upc-a
UPAARQ  , Configure.Symbologies.Linear.UPC Codes, Addenda Required  , CHECK  , UPC-A  ,0,1,0,0, N  , N  ,configure_symbologies_linear_upc_codes.htm#upc-a
UPAADS  , Configure.Symbologies.Linear.UPC Codes, Addenda Separator  , CHECK  , UPC-A  ,0,1,1,0, N  , N  ,configure_symbologies_linear_upc_codes.htm#upc-a
UPADFT  , Configure.Symbologies.Linear.UPC Codes, Default  , DEFCMD  , UPC-A  ,0,0,0,0, N  , N  ,configure_symbologies_linear_upc_codes.htm#upc-a
UPEEN0  , Configure.Symbologies.Linear.UPC Codes, E0 Decoding On  , CHECK  , UPC-E  ,0,1,1,0, N  , N  ,configure_symbologies_linear_upc_codes.htm#upc-e
UPEEN1  , Configure.Symbologies.Linear.UPC Codes, E1 Decoding On  , CHECK  , UPC-E  ,0,1,0,0, N  , N  ,configure_symbologies_linear_upc_codes.htm#upc-e
UPEEXP  , Configure.Symbologies.Linear.UPC Codes, E Expand  , CHECK  , UPC-E  ,0,1,0,0, N  , N  ,configure_symbologies_linear_upc_codes.htm#upc-e
UPECKX  , Configure.Symbologies.Linear.UPC Codes, E Check Digit Transmit  , CHECK  , UPC-E  ,0,1,1,0, N  , N  ,configure_symbologies_linear_upc_codes.htm#upc-e
UPENSX  , Configure.Symbologies.Linear.UPC Codes, E Number System Digit Transmit  , CHECK  , UPC-E  ,0,1,1,0, N  , N  ,configure_symbologies_linear_upc_codes.htm#upc-e
UPEAD2  , Configure.Symbologies.Linear.UPC Codes, E0/E1 2 Digit Addenda  , CHECK  , UPC-E  ,0,1,0,0, N  , N  ,configure_symbologies_linear_upc_codes.htm#upc-e
UPEAD5  , Configure.Symbologies.Linear.UPC Codes, E0/E1 5 Digit Addenda  , CHECK  , UPC-E  ,0,1,0,0, N  , N  ,configure_symbologies_linear_upc_codes.htm#upc-e
UPEARQ  , Configure.Symbologies.Linear.UPC Codes, E0/E1 Addenda Required  , CHECK  , UPC-E  ,0,1,0,0, N  , N  ,configure_symbologies_linear_upc_codes.htm#upc-e
UPEADS  , Configure.Symbologies.Linear.UPC Codes, E0/E1 Addenda Separator  , CHECK  , UPC-E  ,0,1,1,0, N  , N  ,configure_symbologies_linear_upc_codes.htm#upc-e
UPEDFT  , Configure.Symbologies.Linear.UPC Codes, Default  , DEFCMD  , UPC-E  ,0,0,0,0, N  , N  ,configure_symbologies_linear_upc_codes.htm#upc-e
CPNENA  , Configure.Symbologies.Linear.UPC Codes, Decoding On  , CHECK  , UPC-A/EAN-13 Extended Coupon Code  ,0,1,1,0, N  , N  ,configure_symbologies_linear_upc_codes.htm#upc-a/ean-13_extended_coupon_code
E13ENA  , Configure.Symbologies.Linear.EAN Codes, Decoding On  , CHECK  , EAN/JAN-13  ,0,1,1,0, N  , N  ,configure_symbologies_linear_ean_codes.htm#ean/jan-13
E13CKX  , Configure.Symbologies.Linear.EAN Codes, Check Digit Transmit  , CHECK  , EAN/JAN-13  ,0,1,1,0, N  , N  ,configure_symbologies_linear_ean_codes.htm#ean/jan-13
E13AD2  , Configure.Symbologies.Linear.EAN Codes, 2 Digit Addenda  , CHECK  , EAN/JAN-13  ,0,1,0,0, N  , N  ,configure_symbologies_linear_ean_codes.htm#ean/jan-13
E13AD5  , Configure.Symbologies.Linear.EAN Codes, 5 Digit Addenda  , CHECK  , EAN/JAN-13  ,0,1,0,0, N  , N  ,configure_symbologies_linear_ean_codes.htm#ean/jan-13
E13ARQ  , Configure.Symbologies.Linear.EAN Codes, Addenda Required  , CHECK  , EAN/JAN-13  ,0,1,0,0, N  , N  ,configure_symbologies_linear_ean_codes.htm#ean/jan-13
E13ADS  , Configure.Symbologies.Linear.EAN Codes, Addenda Separator  , CHECK  , EAN/JAN-13  ,0,1,1,0, N  , N  ,configure_symbologies_linear_ean_codes.htm#ean/jan-13
E13ISB  , Configure.Symbologies.Linear.EAN Codes, ISBN On  , CHECK  , EAN/JAN-13  ,0,1,0,0, N  , N  ,configure_symbologies_linear_ean_codes.htm#ean/jan-13
E13DFT  , Configure.Symbologies.Linear.EAN Codes, Default  , DEFCMD  , EAN/JAN-13  ,0,0,0,0, N  , N  ,configure_symbologies_linear_ean_codes.htm#ean/jan-13
EA8ENA  , Configure.Symbologies.Linear.EAN Codes, Decoding On  , CHECK  , EAN/JAN-8  ,0,1,1,0, N  , N  ,configure_symbologies_linear_ean_codes.htm#ean/jan-8
EA8CKX  , Configure.Symbologies.Linear.EAN Codes, Check Digit Transmit  , CHECK  , EAN/JAN-8  ,0,1,1,0, N  , N  ,configure_symbologies_linear_ean_codes.htm#ean/jan-8
EA8AD2  , Configure.Symbologies.Linear.EAN Codes, 2 Digit Addenda  , CHECK  , EAN/JAN-8  ,0,1,0,0, N  , N  ,configure_symbologies_linear_ean_codes.htm#ean/jan-8
EA8AD5  , Configure.Symbologies.Linear.EAN Codes, 5 Digit Addenda  , CHECK  , EAN/JAN-8  ,0,1,0,0, N  , N  ,configure_symbologies_linear_ean_codes.htm#ean/jan-8
EA8ARQ  , Configure.Symbologies.Linear.EAN Codes, Addenda Required  , CHECK  , EAN/JAN-8  ,0,1,0,0, N  , N  ,configure_symbologies_linear_ean_codes.htm#ean/jan-8
EA8ADS  , Configure.Symbologies.Linear.EAN Codes, Addenda Separator  , CHECK  , EAN/JAN-8  ,0,1,1,0, N  , N  ,configure_symbologies_linear_ean_codes.htm#ean/jan-8
EA8DFT  , Configure.Symbologies.Linear.EAN Codes, Default  , DEFCMD  , EAN/JAN-8  ,0,0,0,0, N  , N  ,configure_symbologies_linear_ean_codes.htm#ean/jan-8
A25ENA  , Configure.Symbologies.Linear.2 of 5 Codes, Decoding On  , CHECK  , IATA 2/5  ,0,1,0,0, N  , N  ,configure_symbologies_linear_2_of_5_codes.htm#iata_2/5
A25MIN  , Configure.Symbologies.Linear.2 of 5 Codes, Minimum Length  , EDIT  , IATA 2/5  ,1,48,4,0, N  , N  ,configure_symbologies_linear_2_of_5_codes.htm#iata_2/5
A25MAX  , Configure.Symbologies.Linear.2 of 5 Codes, Maximum Length  , EDIT  , IATA 2/5  ,1,48,48,0, N  , N  ,configure_symbologies_linear_2_of_5_codes.htm#iata_2/5
A25DFT  , Configure.Symbologies.Linear.2 of 5 Codes, Default  , DEFCMD  , IATA 2/5  ,0,0,0,0, N  , N  ,configure_symbologies_linear_2_of_5_codes.htm#iata_2/5
I25ENA  , Configure.Symbologies.Linear.2 of 5 Codes, Decoding On  , CHECK  , Interleaved 2/5  ,0,1,1,0, N  , N  ,configure_symbologies_linear_2_of_5_codes.htm#interleaved_2/5
I25CK2  , Configure.Symbologies.Linear.2 of 5 Codes, Check Character  , RADIO1  , Interleaved 2/5  ,0,0, No Check Character  ,No Check Character|Validate but Don't Transmit| Validate and Transmit  , N  , N  ,configure_symbologies_linear_2_of_5_codes.htm#interleaved_2/5
I25MIN  , Configure.Symbologies.Linear.2 of 5 Codes, Minimum Length  , EDIT  , Interleaved 2/5  ,2,80,4,0, N  , N  ,configure_symbologies_linear_2_of_5_codes.htm#interleaved_2/5
I25MAX  , Configure.Symbologies.Linear.2 of 5 Codes, Maximum Length  , EDIT  , Interleaved 2/5  ,2,80,80,0, N  , N  ,configure_symbologies_linear_2_of_5_codes.htm#interleaved_2/5
I25DFT  , Configure.Symbologies.Linear.2 of 5 Codes, Default  , DEFCMD  , Interleaved 2/5  ,0,0,0,0, N  , N  ,configure_symbologies_linear_2_of_5_codes.htm#interleaved_2/5
X25ENA  , Configure.Symbologies.Linear.2 of 5 Codes, Decoding On  , CHECK  , Matrix 2/5  ,0,1,0,0, N  , N  ,configure_symbologies_linear_2_of_5_codes.htm#matrix_2/5
X25MIN  , Configure.Symbologies.Linear.2 of 5 Codes, Minimum Length  , EDIT  , Matrix 2/5  ,1,80,4,0, N  , N  ,configure_symbologies_linear_2_of_5_codes.htm#matrix_2/5
X25MAX  , Configure.Symbologies.Linear.2 of 5 Codes, Maximum Length  , EDIT  , Matrix 2/5  ,1,80,80,0, N  , N  ,configure_symbologies_linear_2_of_5_codes.htm#matrix_2/5
X25DFT  , Configure.Symbologies.Linear.2 of 5 Codes, Default  , DEFCMD  , Matrix 2/5  ,0,0,0,0, N  , N  ,configure_symbologies_linear_2_of_5_codes.htm#matrix_2/5
R25ENA  , Configure.Symbologies.Linear.2 of 5 Codes, Decoding On  , CHECK  , Code 2/5  ,0,1,0,0, N  , N  ,configure_symbologies_linear_2_of_5_codes.htm#code_2/5
R25MIN  , Configure.Symbologies.Linear.2 of 5 Codes, Minimum Length  , EDIT  , Code 2/5  ,1,48,4,0, N  , N  ,configure_symbologies_linear_2_of_5_codes.htm#code_2/5
R25MAX  , Configure.Symbologies.Linear.2 of 5 Codes, Maximum Length  , EDIT  , Code 2/5  ,1,48,48,0, N  , N  ,configure_symbologies_linear_2_of_5_codes.htm#code_2/5
R25DFT  , Configure.Symbologies.Linear.2 of 5 Codes, Default  , DEFCMD  , Code 2/5  ,0,0,0,0, N  , N  ,configure_symbologies_linear_2_of_5_codes.htm#code_2/5
MSIENA  , Configure.Symbologies.Linear.MSI/Plessey, Decoding On  , CHECK  , MSI  ,0,1,0,0, N  , N  ,configure_symbologies_linear_msi_plessey.htm#msi
MSICHK  , Configure.Symbologies.Linear.MSI/Plessey, Check Character  , RADIO1  , MSI  ,0,0, Validate MOD 10 - No Transmit  ,Validate MOD 10 - No Transmit| Validate MOD 10 - Transmit  , N  , N  ,configure_symbologies_linear_msi_plessey.htm#msi
MSIMIN  , Configure.Symbologies.Linear.MSI/Plessey, Minimum Length  , EDIT  , MSI  ,4,48,4,0, N  , N  ,configure_symbologies_linear_msi_plessey.htm#msi
MSIMAX  , Configure.Symbologies.Linear.MSI/Plessey, Maximum Length  , EDIT  , MSI  ,4,48,48,0, N  , N  ,configure_symbologies_linear_msi_plessey.htm#msi
MSIDFT  , Configure.Symbologies.Linear.MSI/Plessey, Default  , DEFCMD  , MSI  ,0,0,0,0, N  , N  ,configure_symbologies_linear_msi_plessey.htm#msi
PLSENA  , Configure.Symbologies.Linear.MSI/Plessey, Decoding On  , CHECK  , Plessey  ,0,1,0,0, N  , N  ,configure_symbologies_linear_msi_plessey.htm#plessey
PLSMIN  , Configure.Symbologies.Linear.MSI/Plessey, Minimum Length  , EDIT  , Plessey  ,4,48,4,0, N  , N  ,configure_symbologies_linear_msi_plessey.htm#plessey
PLSMAX  , Configure.Symbologies.Linear.MSI/Plessey, Maximum Length  , EDIT  , Plessey  ,4,48,48,0, N  , N  ,configure_symbologies_linear_msi_plessey.htm#plessey
PLSDFT  , Configure.Symbologies.Linear.MSI/Plessey, Default  , DEFCMD  , Plessey  ,0,0,0,0, N  , N  ,configure_symbologies_linear_msi_plessey.htm#plessey
TELENA  , Configure.Symbologies.Linear.Other, Decoding On  , CHECK  , Telepen  ,0,1,0,0, N  , N  ,configure_symbologies_linear_other.htm#telepen
TELOLD  , Configure.Symbologies.Linear.Other, Telepen Output  , RADIO1  , Telepen  ,0,1, AIM  ,AIM| Original  , N  , N  ,configure_symbologies_linear_other.htm#telepen
TELMIN  , Configure.Symbologies.Linear.Other, Minimum Length  , EDIT  , Telepen  ,1,60,1,0, N  , N  ,configure_symbologies_linear_other.htm#telepen
TELMAX  , Configure.Symbologies.Linear.Other, Maximum Length  , EDIT  , Telepen  ,1,60,60,0, N  , N  ,configure_symbologies_linear_other.htm#telepen
TELDFT  , Configure.Symbologies.Linear.Other, Default  , DEFCMD  , Telepen  ,0,0,0,0, N  , N  ,configure_symbologies_linear_other.htm#telepen
RSSENA  , Configure.Symbologies.Linear.Other, RSS-14 Decoding On  , CHECK  , RSS-14  ,0,1,1,0, N  , N  ,configure_symbologies_linear_other.htm#rss-14
RSSDFT  , Configure.Symbologies.Linear.Other, RSS-14 Default  , DEFCMD  , RSS-14  ,0,0,0,0, N  , N  ,configure_symbologies_linear_other.htm#rss-14
RSLENA  , Configure.Symbologies.Linear.Other, RSS-14 Limited Code On  , CHECK  , RSS-14  ,0,1,1,0, N  , N  ,configure_symbologies_linear_other.htm#rss-14
RSLDFT  , Configure.Symbologies.Linear.Other, RSS-14 Limited Default  , DEFCMD  , RSS-14  ,0,0,0,0, N  , N  ,configure_symbologies_linear_other.htm#rss-14
RSEENA  , Configure.Symbologies.Linear.Other, RSS Expanded Decoding On  , CHECK  , RSS-14  ,0,1,1,0, N  , N  ,configure_symbologies_linear_other.htm#rss-14
RSEMIN  , Configure.Symbologies.Linear.Other, RSS Expanded Minimum Length  , EDIT  , RSS-14  ,1,80,1,0, N  , N  ,configure_symbologies_linear_other.htm#rss-14
RSEMAX  , Configure.Symbologies.Linear.Other, RSS Expanded Maximum Length  , EDIT  , RSS-14  ,4,74,74,0, N  , N  ,configure_symbologies_linear_other.htm#rss-14
RSEDFT  , Configure.Symbologies.Linear.Other, RSS Expanded Default  , DEFCMD  , RSS-14  ,0,0,0,0, N  , N  ,configure_symbologies_linear_other.htm#rss-14
POSENA  , Configure.Symbologies.Linear.Other, Decoding On  , CHECK  , Posicode  ,0,1,1,0, N  , N  ,configure_symbologies_linear_other.htm#posicode
POSMIN  , Configure.Symbologies.Linear.Other, Minimum Length  , EDIT  , Posicode  ,2,80,4,0, N  , N  ,configure_symbologies_linear_other.htm#posicode
POSMAX  , Configure.Symbologies.Linear.Other, Maximum Length  , EDIT  , Posicode  ,2,80,48,0, N  , N  ,configure_symbologies_linear_other.htm#posicode
POSLIM  , Configure.Symbologies.Linear.Other, PosiCode Limited  , RADIO1  , Posicode  ,0,0, 'B' Limited  ,Disabled|'A' Limited| 'B' Limited  , N  , N  ,configure_symbologies_linear_other.htm#posicode
POSDFT  , Configure.Symbologies.Linear.Other, Default  , DEFCMD  , Posicode  ,0,0,0,0, N  , N  ,configure_symbologies_linear_other.htm#posicode
TRIENA  , Configure.Symbologies.Linear.Other, Decoding On  , CHECK  , Trioptic Code  ,0,1,0,0, N  , N  ,configure_symbologies_linear_other.htm#trioptic_code
PDFENA  , Configure.Symbologies.Stacked Linears  , Decoding On  , CHECK  , PDF417  ,0,1,1,0, N  , N  ,configure_symbologies_stacked_linears.htm#pdf417
PDFGLI  , Configure.Symbologies.Stacked Linears  , Show GLI Blocks  , CHECK  , PDF417  ,0,1,0,0, N  , N  ,configure_symbologies_stacked_linears.htm#pdf417
PDFMIN  , Configure.Symbologies.Stacked Linears  , Minimum Length  , EDIT  , PDF417  ,0,2750,1,0, N  , N  ,configure_symbologies_stacked_linears.htm#pdf417
PDFMAX  , Configure.Symbologies.Stacked Linears  , Maximum Length  , EDIT  , PDF417  ,0,2750,2750,0, N  , N  ,configure_symbologies_stacked_linears.htm#pdf417
PDFDFT  , Configure.Symbologies.Stacked Linears  , Default  , DEFCMD  , PDF417  ,0,0,0,0, N  , N  ,configure_symbologies_stacked_linears.htm#pdf417
PDFDCP  , Configure.Symbologies.Stacked Linears  , Code Page  , COMBOBOX  , PDF 417 Code Page  ,0,0, CP437 (MS-DOS USA)  ,N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|CP1250 (Windows)|CP1251 (Windows)|CP1252 (Windows)|CP1253 (Windows)|CP1254 (Windows)|CP1255 (Windows)|CP1256 (Windows)|CP1257 (Windows)|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|CP437 (MS-DOS USA)|CP737 (MS-DOS)|CP775 (MS-DOS)|CP850 (MS-DOS)|CP852 (MS-DOS)|CP855 (MS-DOS)|CP857 (MS-DOS)|CP866 (MS-DOS)|CP862 (MS-DOS)|CP864 (MS-DOS)|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|ISO 8859-1|ISO 8859-2|ISO 8859-3|ISO 8859-4|ISO 8859-5|ISO 8859-6|ISO 8859-7|ISO 8859-8|ISO 8859-9|ISO 8859-10|ISO 8859-11|ISO 8859-12|ISO 8859-13|ISO 8859-14|ISO 8859-15|N/A|N/A|N/A|N/A|KIO8-U (Ukraine)|KIO8-R (Russian)   , N  , Y  ,configure_symbologies_stacked_linears.htm#pdf_417_code_page
MPDENA  , Configure.Symbologies.Stacked Linears  , Decoding On  , CHECK  , Micro PDF  ,0,1,0,0, N  , N  ,configure_symbologies_stacked_linears.htm#micro_pdf
MPDMIN  , Configure.Symbologies.Stacked Linears  , Minimum Length  , EDIT  , Micro PDF  ,1,366,1,0, N  , N  ,configure_symbologies_stacked_linears.htm#micro_pdf
MPDMAX  , Configure.Symbologies.Stacked Linears  , Maximum Length  , EDIT  , Micro PDF  ,1,366,366,0, N  , N  ,configure_symbologies_stacked_linears.htm#micro_pdf
MPDDFT  , Configure.Symbologies.Stacked Linears  , Default  , DEFCMD  , Micro PDF  ,0,0,0,0, N  , N  ,configure_symbologies_stacked_linears.htm#micro_pdf
MPDDCP  , Configure.Symbologies.Stacked Linears  , Code Page  , COMBOBOX  , Micro PDF Code Page  ,0,0, CP437 (MS-DOS USA)  ,N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|CP1250 (Windows)|CP1251 (Windows)|CP1252 (Windows)|CP1253 (Windows)|CP1254 (Windows)|CP1255 (Windows)|CP1256 (Windows)|CP1257 (Windows)|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|    CP437 (MS-DOS USA)|CP737 (MS-DOS)|CP775 (MS-DOS)|CP850 (MS-DOS)|CP852 (MS-DOS)|CP855 (MS-DOS)|CP857 (MS-DOS)|CP866 (MS-DOS)|CP862 (MS-DOS)|CP864 (MS-DOS)|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|ISO 8859-1|ISO 8859-2|ISO 8859-3|ISO 8859-4|ISO 8859-5|ISO 8859-6|ISO 8859-7|ISO 8859-8|ISO 8859-9|ISO 8859-10|ISO 8859-11|ISO 8859-12|ISO 8859-13|ISO 8859-14|ISO 8859-15|N/A|N/A|N/A|N/A|KIO8-U (Ukraine)|KIO8-R (Russian), N  , N  ,configure_symbologies_stacked_linears.htm#micro_pdf_code_page
COMENA  , Configure.Symbologies.Stacked Linears  , Decoding On  , CHECK  , Composite Code  ,0,1,0,0, N  , N  ,configure_symbologies_stacked_linears.htm#composite_code
COMUPC  , Configure.Symbologies.Stacked Linears  , Enable on UPC/EAN  , CHECK  , Composite Code  ,0,1,0,0, N  , N  ,configure_symbologies_stacked_linears.htm#composite_code
COMMIN  , Configure.Symbologies.Stacked Linears  , Minimum Length  , EDIT  , Composite Code  ,1,2435,1,0, N  , N  ,configure_symbologies_stacked_linears.htm#composite_code
COMMAX  , Configure.Symbologies.Stacked Linears  , Maximum Length  , EDIT  , Composite Code  ,1,2435,2435,0, N  , N  ,configure_symbologies_stacked_linears.htm#composite_code
COMDFT  , Configure.Symbologies.Stacked Linears  , Default  , DEFCMD  , Composite Code  ,0,0,0,0, N  , N  ,configure_symbologies_stacked_linears.htm#composite_code
COMDCP  , Configure.Symbologies.Stacked Linears  , Code Page  , COMBOBOX  , Composite Code Page  ,0,0, CP437 (MS-DOS USA)  ,N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|CP1250 (Windows)|CP1251 (Windows)|CP1252 (Windows)|CP1253 (Windows)|CP1254 (Windows)|CP1255 (Windows)|CP1256 (Windows)|CP1257 (Windows)|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|   CP437 (MS-DOS USA)|CP737 (MS-DOS)|CP775 (MS-DOS)|CP850 (MS-DOS)|CP852 (MS-DOS)|CP855 (MS-DOS)|CP857 (MS-DOS)|CP866 (MS-DOS)|CP862 (MS-DOS)|CP864 (MS-DOS)|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|ISO 8859-1|ISO 8859-2|ISO 8859-3|ISO 8859-4|ISO 8859-5|ISO 8859-6|ISO 8859-7|ISO 8859-8|ISO 8859-9|ISO 8859-10|ISO 8859-11|ISO 8859-12|ISO 8859-13|ISO 8859-14|ISO 8859-15|N/A|N/A|N/A|N/A|KIO8-U (Ukraine)|KIO8-R (Russian), N  , N  ,configure_symbologies_stacked_linears.htm#composite_code_page
16KENA  , Configure.Symbologies.Stacked Linears  , Decoding On  , CHECK  , Code 16K  ,0,1,0,0, N  , N  ,configure_symbologies_stacked_linears.htm#code_16k
16KMIN  , Configure.Symbologies.Stacked Linears  , Minimum Length  , EDIT  , Code 16K  ,1,160,1,0, N  , N  ,configure_symbologies_stacked_linears.htm#code_16k
16KMAX  , Configure.Symbologies.Stacked Linears  , Maximum Length  , EDIT  , Code 16K  ,1,160,160,0, N  , N  ,configure_symbologies_stacked_linears.htm#code_16k
16KDFT  , Configure.Symbologies.Stacked Linears  , Default  , DEFCMD  , Code 16K  ,0,0,0,0, N  , N  ,configure_symbologies_stacked_linears.htm#code_16k
C49ENA  , Configure.Symbologies.Stacked Linears  , Decoding On  , CHECK  , Code 49  ,0,1,1,0, N  , N  ,configure_symbologies_stacked_linears.htm#code_49
C49MIN  , Configure.Symbologies.Stacked Linears  , Minimum Length  , EDIT  , Code 49  ,1,81,1,0, N  , N  ,configure_symbologies_stacked_linears.htm#code_49
C49MAX  , Configure.Symbologies.Stacked Linears  , Maximum Length  , EDIT  , Code 49  ,1,81,81,0, N  , N  ,configure_symbologies_stacked_linears.htm#code_49
C49DFT  , Configure.Symbologies.Stacked Linears  , Default  , DEFCMD  , Code 49  ,0,0,0,0, N  , N  ,configure_symbologies_stacked_linears.htm#code_49
CBFENA  , Configure.Symbologies.Stacked Linears  , Decoding On  , CHECK  , Codablock F  ,0,1,0,0, N  , N  ,configure_symbologies_stacked_linears.htm#codablock_f
CBFMIN  , Configure.Symbologies.Stacked Linears  , Minimum Length  , EDIT  , Codablock F  ,0,2048,1,0, N  , N  ,configure_symbologies_stacked_linears.htm#codablock_f
CBFMAX  , Configure.Symbologies.Stacked Linears  , Maximum Length  , EDIT  , Codablock F  ,0,2048,2048,0, N  , N  ,configure_symbologies_stacked_linears.htm#codablock_f
CBFDFT  , Configure.Symbologies.Stacked Linears  , Default  , DEFCMD  , Codablock F  ,0,0,0,0, N  , N  ,configure_symbologies_stacked_linears.htm#codablock_f
EANEMU  , Configure.Symbologies.Stacked Linears  , EAN-UCC Emulation  , RADIO1  , None  ,0,0, EAN-UCC Emulation Off  , EAN-UCC Emulation Off|128 Emulation|RSS Emulation  , N  , N  ,configure_symbologies_stacked_linears.htm#ean-ucc_emulation
T39ENA  , Configure.Symbologies.Stacked Linears  , Decoding On  , CHECK  , TLC39  ,0,1,0,0,N,N,configure_symbologies_stacked_linears.htm#tlc39
AZTENA  , Configure.Symbologies.2D, Decoding On  , CHECK  , Aztec  ,0,1,1,0, N  , N  ,configure_symbologies_2d.htm#aztec
AZTMIN  , Configure.Symbologies.2D, Minimum Length  , EDIT  , Aztec  ,0,3750,1,0, N  , N  ,configure_symbologies_2d.htm#aztec
AZTMAX  , Configure.Symbologies.2D, Maximum Length  , EDIT  , Aztec  ,0,3750,3750,0, N  , N  ,configure_symbologies_2d.htm#aztec
AZTRUN  , Configure.Symbologies.2D, Runes On  , CHECK  , Aztec  ,0,1,0,0, N  , N  ,configure_symbologies_2d.htm#aztec
AZTDFT  , Configure.Symbologies.2D, Default  , DEFCMD  , Aztec  ,0,0,0,0, N  , N  ,configure_symbologies_2d.htm#aztec
AZTDCP  , Configure.Symbologies.2D, Code Page  , COMBOBOX  , Aztec Code Page  ,0,0, ISO 8859-1  ,N/A|ASCII - USA (ISO 2022-6/ISO646)|ISO 2022 Auto|N/A|N/A|N/A|N/A|N/A|N/A|N/A|   N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|    N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|    N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|    N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|    N/A|ISO 8859-1|ISO 8859-2|ISO 8859-3|ISO 8859-4|ISO 8859-5|ISO 8859-6|ISO 8859-7|ISO 8859-8|ISO 8859-9|    ISO 8859-10|ISO 8859-11|ISO 8859-12|ISO 8859-13|ISO 8859-14|ISO 8859-15|N/A|N/A|N/A|N/A|    KIO8-U (Ukraine)|KIO8-R (Russian)|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|    N/A|ISO 2022-25 (France / Belgium)|ISO 2022-11 (Sweden)|ISO 2022-69 (France / Belgium)|ISO 2022-21 (Germany)|ISO 2022-15 (Italy)|ISO 2022-xx (Switzerland)|ISO 2022-04 (UK)|ISO 2022-xx (Denmark)|ISO 2022-61 (Norway)|    ISO 2022-17 (Spain)|,N,N,configure_symbologies_2d.htm#aztec_code_page
MAXENA  , Configure.Symbologies.2D, Decoding On  , CHECK  , MaxiCode  ,0,1,1,0, N  , N  ,configure_symbologies_2d.htm#maxicode
MAXMIN  , Configure.Symbologies.2D, Minimum Length  , EDIT  , MaxiCode  ,0,150,1,0, N  , N  ,configure_symbologies_2d.htm#maxicode
MAXMAX  , Configure.Symbologies.2D, Maximum Length  , EDIT  , MaxiCode  ,0,150,150,0, N  , N  ,configure_symbologies_2d.htm#maxicode
MAXSCM  , Configure.Symbologies.2D, Structured Carrier Message Only  , CHECK  , MaxiCode  ,0,1,0,0, N  , N  ,configure_symbologies_2d.htm#maxicode
MAXDFT  , Configure.Symbologies.2D, Default  , DEFCMD  , MaxiCode  ,0,0,0,0, N  , N  ,configure_symbologies_2d.htm#maxicode
IDMENA  , Configure.Symbologies.2D, Decoding On  , CHECK  , Data Matrix  ,0,1,1,0, N  , N  ,configure_symbologies_2d.htm#data_matrix
IDMMIN  , Configure.Symbologies.2D, Minimum Length  , EDIT  , Data Matrix  ,0,3116,1,0, N  , N  ,configure_symbologies_2d.htm#data_matrix
IDMMAX  , Configure.Symbologies.2D, Maximum Length  , EDIT  , Data Matrix  ,0,3116,3116,0, N  , N  ,configure_symbologies_2d.htm#data_matrix
IDMDFT  , Configure.Symbologies.2D, Default  , DEFCMD  , Data Matrix  ,0,0,0,0, N  , N  ,configure_symbologies_2d.htm#data_matrix
IDMDCP  , Configure.Symbologies.2D, Code Page  , COMBOBOX  , Data Matrix Code Page  ,0,0, ISO 8859-1  ,N/A|ASCII - USA (ISO 2022-6/ISO646)|ISO 2022 Auto|N/A|N/A|N/A|N/A|N/A|N/A|N/A|   N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|    N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|    N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|    N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|    N/A|ISO 8859-1|ISO 8859-2|ISO 8859-3|ISO 8859-4|ISO 8859-5|ISO 8859-6|ISO 8859-7|ISO 8859-8|ISO 8859-9|    ISO 8859-10|ISO 8859-11|ISO 8859-12|ISO 8859-13|ISO 8859-14|ISO 8859-15|N/A|N/A|N/A|N/A|    KIO8-U (Ukraine)|KIO8-R (Russian)|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|    N/A|ISO 2022-25 (France / Belgium)|ISO 2022-11 (Sweden)|ISO 2022-69 (France / Belgium)|ISO 2022-21 (Germany)|ISO 2022-15 (Italy)|ISO 2022-xx (Switzerland)|ISO 2022-04 (UK)|ISO 2022-xx (Denmark)|ISO 2022-61 (Norway)|    ISO 2022-17 (Spain)|,N,N,configure_symbologies_2d.htm#data_matrix_code_page
QRCENA  , Configure.Symbologies.2D, Decoding On  , CHECK  , QR Code  ,0,1,1,0, N  , N  ,configure_symbologies_2d.htm#qr_code
QRCMIN  , Configure.Symbologies.2D, Minimum Length  , EDIT  , QR Code  ,0,3500,1,0, N  , N  ,configure_symbologies_2d.htm#qr_code
QRCMAX  , Configure.Symbologies.2D, Maximum Length  , EDIT  , QR Code  ,0,3500,3500,0, N  , N  ,configure_symbologies_2d.htm#qr_code
QRCDFT  , Configure.Symbologies.2D, Default  , DEFCMD  , QR Code  ,0,0,0,0, N  , N  ,configure_symbologies_2d.htm#qr_code
NETENA  , Configure.Symbologies.Postal, Postnet Decoding On  , CHECK  , Postal Code  ,0,1,0,0, N  , N  ,configure_symbologies_postal.htm#postal_code
NETCKX  , Configure.Symbologies.Postal, Postnet Check Digit Transmit  , CHECK  , Postal Code  ,0,1,0,0, N  , N  ,configure_symbologies_postal.htm#postal_code
BPOENA  , Configure.Symbologies.Postal, British Postal Code Decoding On  , CHECK  , Postal Code  ,0,1,0,0, N  , N  ,configure_symbologies_postal.htm#postal_code
CANENA  , Configure.Symbologies.Postal, Canadian Postal Code Decoding On  , CHECK  , Postal Code  ,0,1,0,0, N  , N  ,configure_symbologies_postal.htm#postal_code
JAPENA  , Configure.Symbologies.Postal, Japanese Postal Code Decoding On  , CHECK  , Postal Code  ,0,1,0,0, N  , N  ,configure_symbologies_postal.htm#postal_code
AUSENA  , Configure.Symbologies.Postal, Australian Postal Code Decoding On  , CHECK  , Postal Code  ,0,1,0,0, N  , N  ,configure_symbologies_postal.htm#postal_code
KIXENA  , Configure.Symbologies.Postal, KIX (Netherlands) Postal Code Decoding On  , CHECK  , Postal Code  ,0,1,0,0, N  , N  ,configure_symbologies_postal.htm#postal_code
TAGENA  , Configure.Symbologies.Postal, ID-tag (UPU 4-State)  , CHECK  , Postal Code  ,0,1,0,0, N  , N  ,configure_symbologies_postal.htm#postal_code_(2d_only)
4CBENA  , Configure.Symbologies.Postal, 4-CB (4-State Customer Bar Code)  , CHECK  , Postal Code ,0,1,0,0, N  , N  ,configure_symbologies_postal.htm#postal_code_(2d_only)
PLNENA  , Configure.Symbologies.Postal, Decoding On  , CHECK  , Planet Code  ,0,1,0,0, N  , N  ,configure_symbologies_postal.htm#planet_code
PLNCKX  , Configure.Symbologies.Postal, Check Digit Transmit  , CHECK  , Planet Code  ,0,1,0,0, N  , N  ,configure_symbologies_postal.htm#planet_code
CPCENA  , Configure.Symbologies.Postal, Decoding On  , CHECK  , China Post Code  ,0,1,0,0, N  , N  ,configure_symbologies_postal.htm#china_post_code
CPCMIN  , Configure.Symbologies.Postal, Minimum Length  , EDIT  , China Post Code  ,2,80,4,0, N  , N  ,configure_symbologies_postal.htm#china_post_code
CPCMAX  , Configure.Symbologies.Postal, Maximum Length  , EDIT  , China Post Code  ,2,80,80,0, N  , N  ,configure_symbologies_postal.htm#china_post_code
CPCDFT  , Configure.Symbologies.Postal, Default  , DEFCMD  , China Post Code  ,0,0,0,0, N  , N  ,configure_symbologies_postal.htm#china_post_code
KPCENA  , Configure.Symbologies.Postal, Decoding On  , CHECK  , Korean Postal Code  ,0,1,0,0, N  , N  ,configure_symbologies_postal.htm#korean_postal_code
KPCMIN  , Configure.Symbologies.Postal, Minimum Length  , EDIT  , Korean Postal Code  ,2,80,4,0, N  , N  ,configure_symbologies_postal.htm#korean_postal_code
KPCMAX  , Configure.Symbologies.Postal, Maximum Length  , EDIT  , Korean Postal Code  ,2,80,48,0, N  , N  ,configure_symbologies_postal.htm#korean_postal_code
KPCDFT  , Configure.Symbologies.Postal, Default  , DEFCMD  , Korean Postal Code  ,0,0,0,0, N  , N  ,configure_symbologies_postal.htm#korean_postal_code
OCRENA  , Configure.Symbologies.OCR, Type  , RADIO1  , None  ,0,0, OCR Off  ,OCR Off|OCR-A On|OCR-B On|U.S. Currency On|MICR E-13B On| SEMI Font On  , N  , N  ,configure_symbologies_ocr.htm#type
OCRTMP  , Configure.Symbologies.OCR, Template  , BLOCK_STRING  , OCR Templates  ,0,0," ""dddddddd""  ",0, N  , N  ,configure_symbologies_ocr.htm#ocr_templates
OCRGPG  , Configure.Symbologies.OCR, G Variable  , BLOCK_STRING  , OCR Templates  ,0,0," """"  ",0, N  , N  ,configure_symbologies_ocr.htm#ocr_templates
OCRGPH  , Configure.Symbologies.OCR, H Variable  , BLOCK_STRING  , OCR Templates  ,0,0," """"  ",0, N  , N  ,configure_symbologies_ocr.htm#ocr_templates
OCRCHK  , Configure.Symbologies.OCR, Check Character  , BLOCK_STRING  , OCR Templates  ,0,0," """"  ",0, N  , N  ,configure_symbologies_ocr.htm#ocr_templates
OCRDFT  , Configure.Symbologies.OCR, Default  , DEFCMD  , OCR Templates  ,0,0,0,0, N  , N  ,configure_symbologies_ocr.htm#ocr_templates
232DFT  , Configure.Communications  , Default  , DEFCMD  , All RS-232 Settings  ,0,0,0,0, N  , N  ,configure_communications.htm#all_rs-232_settings
232BAD  , Configure.Communications  , Baud Rate  , RADIO2  , None  ,0,0,38400,N/A|N/A|N/A|N/A|N/A|9600|19200|38400|57600|115200, N  , Y  ,configure_communications.htm#baud_rate
232WRD  , Configure.Communications  , Word Format  , RADIO2  , None  ,0,0, N 8 1  ,N 7 1|N 7 2|N 8 1|E 7 1|E 7 2|E 8 1|O 7 1|O 7 2|O 8 1  , N  , N  ,configure_communications.htm#word_format
232CTS  , Configure.Communications  , RTS/CTS Hardware Flow Control  , RADIO1  , None  ,0,0, Off  , Off|On|N/A  , N  , Y  ,configure_communications.htm#rts/cts_hardware_flow_control
232XON  , Configure.Communications  , XON/XOFF Software Flow Control  , CHECK  , RS-232 Flow Control  ,0,1,0,0, N  , N  ,configure_communications.htm#rs-232_flow_control
232ACK  , Configure.Communications  , ACK/NAK Software Flow Control  , CHECK  , RS-232 Flow Control  ,0,1,0,0, N  , N  ,configure_communications.htm#rs-232_flow_control
232LPT  , Configure.Communications  , RS-232 Receiver Time-Out (sec)  , EDIT  , Low Power  ,0,300,0,0, N  , Y  ,configure_communications.htm#low_power
USBCTS  , Configure.Communications  , CTS Enable  , CHECK  , USB COM Port Emulation  ,0,1,0,0, N  , Y  ,configure_communications.htm#usb_com_port_emulation
USBACK  , Configure.Communications  , ACK Enable  , CHECK  , USB COM Port Emulation  ,0,1,0,0, N  , Y  ,configure_communications.htm#usb_com_port_emulation
USBSER  , Configure.Communications  , USB COM Port Emulation Serial Number  , RADIO1  , None  ,0,0, Enable  ,Disable| Enable  , N  , N,configure_communications.htm#usb_com_port_emulation_Sno
SERWDG  , Configure.Communications  , Serial Wedge Output  , RADIO1  , None  ,0,0, P1  ,Both P1 and P2|P1|P2  , N  , N  ,configure_communications.htm#serial_wedge_output
RTLSCN  , Configure.Interfaces , IBM 4683 Scanner Port  , RADIO1  , None  ,0,0, Port 5B  ,Port 5B|Port 9B HHBCR1|Port 9B HHBCR2| Port 17  , N  , N  ,configure_interfaces.htm#ibm_4683_Scanner_Port
RTLBCD  , Configure.Interfaces , BCD Output  , CHECK  , USB SurePos  ,0,1,0,0, N  , Y  ,configure_interfaces.htm#usb_surepos
PAP232  , Configure.Interfaces , RS-232  , COMMAND  , Plug && Play  ,0,0,0,0, N  , N  ,configure_interfaces.htm#plug_&&_play
PAP_AT  , Configure.Interfaces , IBM-AT Compatible  , COMMAND  , Plug && Play  ,0,0,0,0, N  , N  ,configure_interfaces.htm#plug_&&_play
PAP_XT  , Configure.Interfaces , IBM-XT Compatible  , COMMAND  , Plug && Play  ,0,0,0,0, N  , N  ,configure_interfaces.htm#plug_&&_play
PAPPS2  , Configure.Interfaces , IBM-PS2 Compatible  , COMMAND  , Plug && Play  ,0,0,0,0, N  , N  ,configure_interfaces.htm#plug_&&_play
PAPWM1  , Configure.Interfaces , Wand Emu Code 39  , COMMAND  , Plug && Play  ,0,0,0,0, N  , N  ,configure_interfaces.htm#plug_&&_play
PAPWM2  , Configure.Interfaces , Wand Emu Same Code  , COMMAND  , Plug && Play  ,0,0,0,0, N  , N  ,configure_interfaces.htm#plug_&&_play
PAPLTD  , Configure.Interfaces , Laptop Direct Connect  , COMMAND  , Plug && Play  ,0,0,0,0, N  , N  ,configure_interfaces.htm#plug_&&_play
PAPP5B  , Configure.Interfaces , IBM 4683 Port 5B  , COMMAND  , Plug && Play  ,0,0,0,0, N  , N  ,configure_interfaces.htm#plug_&&_play
PAP9B1  , Configure.Interfaces , IBM 4683 Port 9B HHBCR1  , COMMAND  , Plug && Play  ,0,0,0,0, N  , N  ,configure_interfaces.htm#plug_&&_play
PAP9B2  , Configure.Interfaces , IBM 4683 Port 9B HHBCR2  , COMMAND  , Plug && Play  ,0,0,0,0, N  , N  ,configure_interfaces.htm#plug_&&_play
PAPP17  , Configure.Interfaces , IBM 4683 Port 17  , COMMAND  , Plug && Play  ,0,0,0,0, N  , N  ,configure_interfaces.htm#plug_&&_play
PAP124  , Configure.Interfaces , PC USB Keyboard  , COMMAND  , Plug && Play  ,0,0,0,0, N  , N  ,configure_interfaces.htm#plug_&&_play
PAP125  , Configure.Interfaces , Mac USB Keyboard  , COMMAND  , Plug && Play  ,0,0,0,0, N  , N  ,configure_interfaces.htm#plug_&&_play
PAPSPH  , Configure.Interfaces , USB IBM SurePos Hand Held  , COMMAND  , Plug && Play  ,0,0,0,0, N  , N  ,configure_interfaces.htm#plug_&&_play
PAPSPT  , Configure.Interfaces , USB IBM SurePos Table Top  , COMMAND  , Plug && Play  ,0,0,0,0, N  , N  ,configure_interfaces.htm#plug_&&_play
PAP131  , Configure.Interfaces , USB HID POS  , COMMAND  , Plug && Play  ,0,0,0,0, N  , N  ,configure_interfaces.htm#plug_&&_play
PAPOPS  , Configure.Interfaces , OPOS  , COMMAND  , Plug && Play  ,0,0,0,0, N  , N  ,configure_interfaces.htm#plug_&&_play
VPS2_1  , Configure.Interfaces , French IBM-PS2 Compatible  , COMMAND  , Plug && Play  ,0,0,0,0, N  , N  ,configure_interfaces.htm#plug_&&_play
TERMID  , Configure.Interfaces , Terminal ID  , COMBOBOX  , Terminal Interface  ,0,0, RS-232  ,RS-232|IBM PC XT|IBM PS/2 25 30 77DX2|IBM PC AT Compatible|N/A|DEC VT 510 520 525 PC Keyboard; Esprit; SiliconGraphics|IBM 102 Key Terminal|IBM 122 Key Terminal (3179-1  3191 3192 3471 3472 3194 3151)|IBM 122 Key Terminal (3196 3197 3476 3477 3482 3486)|N/A|\
    N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|\
    N/A|N/A|N/A|HP Vectra (AT Compatible)|IBM 122 Key Terminal 3180|Telex (88 Key)|N/A|N/A|N/A|N/A|\
    N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|\
    N/A|N/A|N/A|N/A|N/A|Telex (102 Key)|Telex (122 Key)|N/A|N/A|N/A|\
    RS-232 Serial Wedge|IBM 468X 469X|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|\
    N/A|Wand Emulation Code 39|N/A|N/A|Wand Emulation Same Code|N/A|N/A|N/A|N/A|N/A|\
    N/A|Decision Data 3496 3497 (122 keys)|N/A|N/A|N/A|N/A|N/A|N/A|N/A|N/A|\
    N/A|N/A|N/A|N/A|Decision Data 3496 3497 (102 keys)|N/A|N/A|N/A|N/A|N/A|\
    Heath Zenith (AT Compatible)|N/A|N/A|N/A|N/A|N/A|N/A|IBM Thinkpad PS2|N/A|N/A|\
    N/A|N/A|Japanese Keyboard Wedge|NEC 98xx Series|DEC VT510 LK411 Keyboard|N/A|IBM Thinkpad AT|N/A|N/A|N/A|\
    N/A|N/A|Telex (88 Key) Data Entry|N/A|IBM 3180 (122 Key) Data Entry|N/A|N/A|N/A|N/A|N/A|\
    Citos/Unisys KB4|Citos/Unisys KB5|N/A|N/A|USB HID Keyboard for PC|USB HID Keyboard for MAC|N/A|N/A|IBM USB POS Handheld (SurePos)|IBM USB POS Tabletop (SurePos)|\
    USB serial port emulation|USB HID POS|N/A|N/A|USB HID Japanese Keyboard for PC, N  , Y  ,configure_interfaces.htm#terminal_interface
CIDNEW  , Data Formatting  , Format  , UNUSED  , Data Formatter  ,0,0,0,0, N  , N  ,data_formatting.htm#data_formatter
DFMBK3  , Data Formatting  , Format  , UNUSED  , Data Formatter  ,0,0,0,0, N  , N  ,data_formatting.htm#data_formatter
DFM_EN  , Data Formatting  , Formatter On  , UNUSED  , Data Formatter  ,0,0,1,Off|On| Required  , N  , N  ,data_formatting.htm#data_formatter
DFMCA3  , Data Formatting  , Format Clear All  , UNUSED  , Data Formatter  ,0,0,0,0, N  , N  ,data_formatting.htm#data_formatter
DFMCL3  , Data Formatting  , Format Clear One  , UNUSED  , Data Formatter  ,0,0,0,0, N  , N  ,data_formatting.htm#data_formatter
DFMDF3  , Data Formatting  , Format Default  , UNUSED  , Data Formatter  ,0,0,0,0, N  , N  ,data_formatting.htm#data_formatter
DFMSIZ  , Data Formatting  , Format Size  , UNUSED  , Data Formatter  ,0,0,0,0, N  , N  ,data_formatting.htm#data_formatter
DFMCMD  , Data Formatting  , Reports Supported Format Cmds  , UNUSED  , Data Formatter  ,0,1,1,0, N  , N  ,data_formatting.htm#data_formatter
PREBK2  , Prefix/Suffix  , Prefix  , UNUSED  , Prefix  ,0,0,0,0, N  , N  ,prefix_suffix.htm#prefix
PRE_EN  , Prefix/Suffix  , Prefix On  , UNUSED  , Prefix  ,0,1,1,0, N  , N  ,prefix_suffix.htm#prefix
PRECA2  , Prefix/Suffix  , Prefix Clear All  , UNUSED  , Prefix  ,0,0,0,0, N  , N  ,prefix_suffix.htm#prefix
PRECL2  , Prefix/Suffix  , Prefix Clear One  , UNUSED  , Prefix  ,0,0,0,0, N  , N  ,prefix_suffix.htm#prefix
PREDF2  , Prefix/Suffix  , Prefix Default  , UNUSED  , Prefix  ,0,0,0,0, N  , N  ,prefix_suffix.htm#prefix
PRESIZ  , Prefix/Suffix  , Prefix Size  , UNUSED  , Prefix  ,0,0,0,0, N  , N  ,prefix_suffix.htm#prefix
SUFBK2  , Prefix/Suffix  , Suffix  , UNUSED  , Suffix  ,0,0, 990d  ,0, N  , N  ,prefix_suffix.htm#suffix
SUF_EN  , Prefix/Suffix  , Suffix On  , UNUSED  , Suffix  ,0,1,1,0, N  , N  ,prefix_suffix.htm#suffix
SUFCA2  , Prefix/Suffix  , Suffix Clear All  , UNUSED  , Suffix  ,0,0,0,0, N  , N  ,prefix_suffix.htm#suffix
SUFCL2  , Prefix/Suffix  , Suffix Clear One  , UNUSED  , Suffix  ,0,0,0,0, N  , N  ,prefix_suffix.htm#suffix
SUFDF2  , Prefix/Suffix  , Suffix Default  , UNUSED  , Suffix  ,0,0,0,0, N  , N  ,prefix_suffix.htm#suffix
SUFSIZ  , Prefix/Suffix  , Suffix Size  , UNUSED  , Suffix  ,0,0,0,0, N  , N  ,prefix_suffix.htm#suffix
FACTRY  , Factory Test  , factory test bar code  , UNUSED  , --  ,0,0,0,0, N  , N  ,factory_test.htm#--
VISMNU  , Visual Menu  , vis menu bar code  , UNUSED  , --  ,0,0,0,0, N  , N  ,visual_menu.htm#--
PAPCLN  , Clone Slave  , ---  , UNUSED  , --  ,0,0,0,0, N  , N  ,clone_slave.htm#--
TERMID  ,Interfaces, Terminal ID  ,UNUSED, Terminal Interface  ,0,0, RS-232  ,RS-232|IBM PC XT|IBM PS/2 25 30 77DX2|IBM PC AT Compatible|DEC VT 220 320 330 340 420|DEC VT 510 520 525 PC Keyboard; Esprit; SiliconGraphics|IBM 102 Key Terminal|IBM 122 Key Terminal (3179-1  3191 3192 3471 3472 3194 3151)|IBM 122 Key Terminal (3196 3197 3476 3477 3482 3486)|Harris H180/H191 122 keys|\
    IBM 122 keys 3178|IBM 122 keys 3278|N/A|Wyse 30 35|Wyse 55 60 99FT 120 150 160 325 370 (ASCII)|Wyse 55 60 99FT 120 150 160 325 370 (ANSI)|Wyse 85 185|Wyse PC AT|Wyse 55 60 120 150 160 370 (Enhanced PC)|Comterm  6178|\
    HP 700/98/92/44|Esprit III|IBM 5291-2|HP Vectra (AT Compatible)|IBM 122 Key Terminal 3180|Telex (88 Key)|Human Designed Systems HDS 2000|Human Designed Systems HDS 3200|N/A|N/A|\
    DDC 3596/97|HP 700/43|HP 700/32|HP 700/x|Siemens 9758 (German only)|Bull BDS-7  Honeywell HDS-7|Telvideo 955 965|Telex general 109 key|Qume  ENHANCED PC|N/A|\
    DDC 3761/91|Bull Questar 310 KB2101|Bull Questar 310 KB3105|N/A|Data Point 8220 8242|Telex (102 Key)|Telex (122 Key)|Falco 5220|N/A|Apple MAC|\
    RS-232 Serial Wedge|IBM 468X 469X|OCIA|N/A|N/A|N/A|N/A|N/A|N/A|N/A|\
    N/A|Wand Emulation Code 39|Microterm 5510|I/O Marketing 1181 1196 1197 2196 2476 2477 2510 2576 2596 (102 keys)|Wand Emulation Same Code|NOKIA KB-100|NOKIA VDU-220|Link 125|Data General DG216/7|DATA GENERAL MT-5220 FOR MEDITECH (AT)|\
    NCR C_ITOH 324|Decision Data 3496 3497 (122 keys)|ADI DT-1496|Decision Data 3776 3777 (122 keys)|Qume  ASCII|Burroughs K5|I/O Marketing 1181 1196 1197 2196 2476 2477 2510 2576 2596 (122 keys)|ICL DRS 300|Sherwood 6030-ST|HP700/60|\
    SAI-220E|Unisys SVT 1120|Qume  ANSI|Decision Data 3776 3777 (102 keys)|Decision Data 3496 3497 (102 keys)|C_ITOH-326|SUN SPARC STATION 1+|N/A|N/A|HHLC Non Decoded Output Laser Emulation|\
    Heath Zenith (AT Compatible)|N/A|CLI|N/A|DATA POINT 7352|IBM-5530 (AT-Type) W/TDOS|HP 700/44|IBM Thinkpad PS2|N/A|Any Terminal|\
    IO 1181 (83 keys)|Wyse 520|Japanese Keyboard Wedge|NEC 98xx Series|DEC VT510 LK411 Keyboard|N/A|IBM Thinkpad AT|N/A|N/A|N/A|\
    N/A|N/A|Telex (88 Key) Data Entry|N/A|IBM 3180 (122 Key) Data Entry|Comterm 6178 DataEntry|N/A|N/A|N/A|Citos/Unisys KB100|\
    N/A|N/A|Burroughs K4|50 Key IBM|USB HID Keyboard for PC|USB HID Keyboard for MAC|N/A|N/A|IBM USB POS Handheld (SurePos)|IBM USB POS Tabletop (SurePos)|\
    USB serial port emulation|USB HID POS|N/A|N/A, N  , Y  ,interfaces.htm#terminal_interface
